Output to serial in the format:

CLEARDATA

LABEL, <col1>, <col2>

In loop

DATA, <data1>, <data2>

DATA,<data1>,<data2>

Etc

Appears as

|  |  |
| --- | --- |
| Col1 | Col2 |
| Data1 | Data2 |
| Data1 | Data2 |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

Can set rows n cols

ROW,SET,n